{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":123,"n_cols":7,"rows_kept":123,"cut":false,"hidden":false,"merged":[]}
[]
[null,"C345","C327","C330","C332","C337","C362"]
["Overall operating height"]
["Overall operating height with foundry/excavating bucket short lip (in. (mm)) ","161.4 (4100)","155.6 (3953)","151.4 (3845)","160.2 (4068)","160.2 (4068)","_"]
["Overall operating height with low profile/standard lip bucket (in. (mm)) ","165.6 (4207)","159.8 (4059)","155.6 (3952)","164.4 (4176)","164.4 (4176)","176.5 (4483)"]
["Overall operating height with low profile extended/long lip bucket (in. (mm)) ","170.4 (4329)","164.6 (4148)","160.6 (4080)","169.2 (4298)","169.2 (4298)","189.6 (4816)"]
["Height to"]
["Bucket hinge pin (in. (mm)) ","131.6 (3342)","125 (3178)","121 (3.07)","131.1 (3330)","131.1 (3330)","140.2 (3562)"]
["Top of ROPS (in. (mm)) ","80.4 (2043)","78.7 (1998)","78.7 (1.99)","80.4 (2043)","80.4 (2043)","84.6 (2150)"]
["Bottom of level bucket, fully raised (in. (mm)) ","123.2 (3129)","117.1 (2976)","114.3 (2902)","123.0 (3125)","123.0 (3125)","133.3 (3386)"]
["Overall length"]
["Overall length without attachment with coupler (in. (mm)) ","120.2 (3054)","104.8 (2662)","105.7 (2.68)","117.3 (2979)","117.0 (2972)","129.5 (3290)"]
["Overall length with foundry excavation bucket on ground (in. (mm)) ","144.6 (3673)","129.6 (3292)","131.4 (3338)","141.7 (3598)","141.1 (3592)","_"]
["Overall length with low profile bucket (in. (mm)) ","148.8 (3781)","133.4 (3388)","135.4 (3440)","147 (3734)","146.7(3727)","159.1 (4041)"]
["Overall length with low profile extended bucket (in. (mm)) ","153.7 (3904)","138.3 (3512)","140.5 (3569)","150.8 (3830)","150.5 (3823)","172.7 (4386)"]
["Dump"]
["Dump angle (degrees) ",45.3,38.1,51.9,55,55,46.1]
["Dump height with foundry/excavating bucket short lip (in. (mm)) ","104.1 (2645) @ 45°","100.6 (2556) @ 38.1°","94.7 (2405) @ 45°","104.5 (2655) @ 45°","104.5 (2655) @ 45°","109 (2768)"]
["Dump height with low profile/standard lip bucket (in. (mm)) ","101.1 (2568) @ 45°","98.0 (2488) @ 38.1°","91.7 (2330) @ 45°","101.6 (2581) @ 45°","101.6 (2581) @ 45°","99.2 (2519)"]
["Dump reach (max height) (in. (mm)) ","31.6 (802) @ 45°","22.3 (568) @ 38.1°","34.7 (882) @ 45°","37 (941) @ 45°","37 (941) @ 45°","39 (990)"]
["Maximum attachment rollback"]
["Bucket on ground (degrees) ",32,31,34.4,33,33,30]
["Bucket at full height (degrees) ",83.1,99,87.6,85,85,84]
["Track and clearance"]
["Track on ground (in. (m)) ","64.5 (1639)","55.9 (1419)","56 (1.42)","64.5 (1.639)","64.5 (1639)","66 (1677)"]
["Ground clearance (bottom of belly pan) (in. (m)) ","9.6 (244)","8 (203)","8.1 (0.20)","9.6 (0.244)","9.6 (244)","12.6 (321)"]
["Angle of departure (degrees) ",32,32,32,32,32,38]
["Clearance circle"]
["Clearance circle without bucket (in. (mm)) ","57.7 (1465)","52.3 (1346)","54.3 (1379)","56.2 (1482)","56.2 (1482)","67.4 (1712)"]
["Clearance circle with foundry bucket in carry position (in. (mm)) ","88 (2234) with 78\" (1981 mm) bucket","82.2 (2187) with 72\" (1829 mm) bucket","84.2 (2139) with 66” (1676 mm) heavy-duty dirt bucket","86.6 (2200) with 78” (1981 mm) bucket","86.6 (2200) with 78” (1981 mm) bucket","_"]
["Clearance circle with low profile bucket on ground (in. (mm)) ","91.8 (2331) with 78\" (1981 mm) bucket","85.8 (2181) with 72\" (1829 mm) bucket","87.9 (2233) with 66” (1676 mm) heavy-duty dirt bucket","90.4 (2297) with 78” (1981 mm) bucket","90.4 (2297) with 78” (1981 mm) bucket","_"]
["Clearance circle with extended low profile on ground (in. (mm)) ","96.2 (2444) with 78\" (1981 mm) bucket","90.4 (2297) with 72\" (1829 mm) bucket","92.5 (2350) with 66” (1676 mm) heavy-duty dirt bucket","94.8 (2409) with 78” (1981 mm) bucket","94.8 (2409) with 78” (1981 mm) bucket","_"]
["Clearance circle rear (in. (mm)) ","67.9 (1725)","59.1 (1501)","59.9 (1523)","67 (1702)","67 (1702)","114 (2913)"]
["Track gauge (in. (mm)) ","58.6 (1488)","53.4 (1356)","53.4 (1356)","58.6 (1488)","58.6 (1488)","_"]
["Overall width (in. (mm)) ","76.5 (1943)","65.9 (1676)","65.9 (1676)","76.5 (1943)","76.5 (1943)","78.3 (1988)"]
["Engine"]
["Manufacturer/model ","FPT / F5BFL413E*B002*","FPT / F5H FL463A","Perkins 404F-E22TA","FPT / F5H FL463A*G001","FPT / F5BFL463A*G001","FPT / F5BFL413D*C005"]
["Type ","Diesel 4-stroke, turbo, D.I.","Diesel 4-stroke, turbo, D.I.","Diesel 4-stroke, Turbo, D.I.","Diesel 4-stroke, turbo, D.I.","Diesel 4-stroke, turbo, D.I.","Diesel, 4-stroke, turbo, D.I."]
["Cylinder ",4,4,4,4,4,4]
["Bore/stroke (in. (mm)) ","3.9 x 4.3 (99 x 110)","3.9 x 4.3 (99 x 109)","3.31 x 3.94 (84 x 100)","3.9 x 4.3 (99 x 110)","3.9 x 4.3 (99 x 110)","3.9 x 4.3 (99 x 110)"]
["Displacement (in.³ (L)) ","207 (3.4)","207 (3.4)","135 (2.2)","207 (3.4)","207.5 (3.4)","207 (3.4)"]
["Fuel injection ","HPCR Direct","HPCR Direct","HPCR Direct","HPCR Direct","HPCR Direct","HPCR Direct"]
["Fuel ","#2 Diesel","#2 Diesel","#2 Diesel","#2 Diesel","#2 Diesel","#2 Diesel"]
["Fuel filter ","Pre-filter 99.8% @ 30 microns, Main filter 95% @ 4 microns","Pre-spin on 30 microns Main-spin on 4 microns","Pre-filter Beta (30) = 200/spin-on, Main filter Beta (4) = 20/spin-on","Pre-spin on 30 microns Main-spin on 4 microns","Pre-filter 99.8% @ 30 microns, Main filter 95% @ 4 microns","Pre-filter Spin on, Beta (30) = 200, Main filter Spin on, Beta (4) > 50, Beta (6) > 200"]
["Air intake ","Turbocharged Aftercooled with external EGR and SCR","Turbocharged with external EGR","Turbocharged with waste gate EGR","Turbocharged Aftercooled with external EGR","Turbocharged Aftercooled with external EGR","Turbocharged Aftercooled with external EGR and SCR"]
["Cooling ","Liquid","Liquid","Liquid","Liquid","Liquid","Liquid"]
["Engine speeds"]
["High idle - no load (rpm) ","2500 +/- 25","2500 +/- 25","2,850 +/- 25","2500 +/- 25","2500 +/- 25","2500 +/- 25"]
["Rated - full load (rpm) ",2500,2500,"2,800",2500,2500,2500]
["Low idle (rpm) ","1150 +/- 25","1150 +/- 25","1,200 +/- 50","1150 +/- 25","1150 +/- 25","1150 +/- 50"]
["Horsepower per SAE J1349"]
["Gross HP  ","90 HP (67 kW)","74 HP (55 kW)","67 HP (50 kW)","74 HP (55 kW)","74 HP (55 kW)","114 HP (85 kW)"]
["Net Horsepower (hp (kW)) ","84 (63) @ 2500 rpm","68 (51) @ 2500 rpm","64 (47.7) @ 2,800 rpm","68 (51) @ 2500 rpm","68 (51) @ 2500 rpm","114 (85) @ 2500"]
["Peak torque (lb.-ft. (Nm)) ","282 (383) @ 1400 rpm","232 (314) @ 1400 rpm","153 (208) @ 1,800 rpm","232 (314) @ 1400 rpm","232 (314) @ 1400 rpm","339 (460) @ 1400"]
["Drive pump electro hydraulic"]
["Pump to engine ratio ",0.0423611111111111,0.0423611111111111,0.0423611111111111,0.0423611111111111,0.0423611111111111,0.0423611111111111]
["Displacement (in.³ (cm³)) ","2.75 (45)","2.75 (45)","2.75 (45)","2.75 (45)","2.75 (45)","49.1 (3)"]
["Flow (gpm (Lpm)) ","29.4 (111)","24.2 (91.5)","30.6 (115.9)","24.2 (91.5)","28.8 (109)","40 (10.5)"]
["Charge pressure (psi (bar)) ","360 (24.5)","362 (24.5)","362 (25)","362 (24.5)","362 (24.5)","377 (26)"]
["System relief (psi (bar)) ","5220 (360)","5220 (360)","5,220 (360)","5220 (360)","5220 (360)","5802 (400)"]
["Control ","Mechanical or Electro hydraulic","Mechanical or Electro hydraulic","Electro hydraulic","Mechanical or Electro hydraulic","Mechanical or Electro hydraulic","Electro hydraulic"]
["Drive motors"]
["Effective Max displacement (in.³ (cm³)) ","3.10 (50.9)","67 (1098)","3.10 (50.9)","3.10 (50.9)","3.10 (50.9)","3.28 (53.8)"]
["Effective Displacement opt high speed (in.³ (cm³)) ","–","43.6 (714)","43.6 (714)","-","–","–"]
["Speed @ high idle engine (rpm) ",103,103,103,103,103,50]
["Speed @ optional high speed (rpm) ",156,156,156,156,156,100]
["Torque @ max displ. and relief pressure (lb.-ft. (Nm)) ","4654 (6310)","4654 (6310)","4654 (6310)","4654 (6310)","4654 (6310)","4840 (6562)"]
["Travel speed"]
["Low range (mph (kph)) ","5.5 (8.9)","5.5 (8.9)","5.8 (9.2)","5.5 (8.9)","5.5 (8.9)","5 (8)"]
["High range (mph (kph)) ","8.0 (12.9)","8.0 (12.9)","8.9 (14.2)","8.0 (12.9)","8.0 (12.9)","8.7 (14)"]
["Final drive ","Planetary gearbox with 2-speed motor","Planetary gearbox with 2-speed motor","Planetary gearbox with 2-speed motor","Planetary gearbox with 2-speed motor","Planetary gearbox with 2-speed motor","Planetary gearbox with 2-speed motor"]
["Parking brake"]
["Type ","Spring applied, hydraulic release disc","Spring applied, hydraulic release disc","Spring applied, hydraulic release multiple disc","Spring applied, hydraulic release disc","Spring applied, hydraulic release disc","Spring applied, hydraulic released multi plet wet disc"]
["Engagement ","Depress on/off brake button on instrument panel, disconnect lapbelt, get off seat, or stop engine","Depress on/off brake button on instrument panel, disconnect lapbelt, get off seat, or stop engine","Depress on/off brake button on handle or instrument panel, raise seat bar, get off seat or stop engine","Depress on/off brake button on instrument panel, disconnect lapbelt, get off seat, or stop engine","Depress on/off brake button on instrument panel, disconnect lapbelt, get off seat, or stop engine","Depress on/off brake button on instrument panel, disconnect lapbelt, get off seat, or stop engine"]
["Undercarriage"]
["System ","Zig Zag Pattern","Zig Zag Pattern","Zig Zag Pattern","Zig Zag Pattern","Zig Zag Pattern","H-Pattern"]
["Idlers / rollers per side ","2025-02-04","2025-02-03","2025-02-03","2025-02-04","2025-02-04","2025-02-06"]
["Ground pressure"]
["PSI (bar) (with spec belt) ","4.4 (0.30)","5.9 (0.41)","5.9 (0.41)","4.2 (0.29)","4.2 (0.29)","6.1 (0.43)"]
["Pumps"]
["Type ","Gear","Gear","Gear","Gear","Gear","Tandem Pump, Integral"]
["Displacement standard aux. (in.³ (cm³)) ","2.23 (36.6)","2.23 (36.6)","1.7 (27.8)","2.23 (36.6)","2.23 (36.6)","3.7 (60)"]
["Displacement high flow aux. (in.³ (cm³)) ","1.45 (23.7)",".76 (12.5)","-","1.24 (20.4)","1.24 (20.4)","3.7 (60)"]
["Standard pump flow (gpm (Lpm)) ","24.2 (91.5)","24.2 (91.5)","24.2 (91.5)","24.2 (91.5)","24.2 (91.5)","10.5 (40)"]
["Optional high flow (gpm (Lpm)) ","39.9 (150.8)","32.4 (122.6)","-","37.6 (142.5)","37.6 (142.5)","41.6 (154.5)"]
["Enhanced high flow (gpm (Lpm)) ","35 (132.5)","_","-","-","_","41.6 (154.5)"]
["Loader control valve"]
["Type ","3 spool / open center / series","3 spool / open center / series","3 spool / open center / series","3 spool / open center / series","3 spool / open center / series","3 spool / closed-center load sensing"]
["Standard relief pressure (psi (bar)) ","3,450 (237)","3046 (210)","3046 (210)","3,046 (210)","3,046 (210)","3,450 (237)"]
["Enhanced high flow relief pressure (psi (bar)) ","4000 (276)","_","-","-","_","4100 (283)"]
["Hydraulic filter ","6 microns / spin on","6 microns / spin on","6 microns / spin on","6 microns / spin on","6 microns / spin on","6 microns / spin on"]
["Lift cylinder"]
["Bore diameter (in. (mm)) ","2.75 (69.8)","2.5 (63.5)","2.6 (63.5)","2.5 (63.5)","2.75 (69.85)","3.25 (82.5)"]
["Rod diameter (in. (mm)) ","1.75 (44.5)","1.75 (44.5)","1.75 (44.5)","1.75 (44.5)","1.75 (44.5)","2.25 (57.1)"]
["Stroke (in. (mm)) ","35.7 (908)","31.69 (804.9)","26.8 (681)","33.5 (851.9)","34.9 (886.5)","38.8 (985)"]
["Closed length (in. (mm)) ","53.9 (1369.1)","45.59 (1158.0)","38.6 (982)","46.9 (1192)","47.4 (1205)","59.6 (1515)"]
["Bucket cylinders"]
["Bore diameter (in. (mm)) ","3.0 (76.2)","2.75 (69.9)","34.9 (69.9)","3.0 (76.2)","3.0 (76.2)","3.25 (82.5)"]
["Rod diameter (in. (mm)) ","1.5 (38.1)","1.38 (34.9)","1.38 (34.9)","1.5 (38.1)","1.5 (38.1)","1.75 (44.5)"]
["Stroke (in. (mm)) ","15.9 (405)","16.14 (410)","16.1 (410)","16.14 (410)","16.14 (410)","19.7 (500)"]
["Closed length (in. (mm)) ","24.3 (617)","24.02 (610)","24.0 (610)","24 (610)","24 (610)","31.5 (800)"]
["Rated operating load"]
["50% tip (lbs. (kg)) ","4500 (2045)","2700 (1225)","3000 (1364)","3200 (1451)","3700 (1678)","6200 (2812)"]
["35% tip (lbs. (kg)) ","3150 (1432)","1890 (860)","2100 (955)","2240 (1018)","2590 (1178)","4340 (1969)"]
["Tipping load (lbs. (kg)) ","9000 (4091)","5400 (2449)","6000 (2727)","6400 (2902)","7400 (3357)","12,500 (5670)"]
["Breakout forces"]
["Lift cylinder (lbs. (kN)) ","7562 (33.6)","6260 (27)","3450 (15.3)","4840 (21.5)","6110 (27.2)","12,084 (53.8)"]
["Bucket cylinder (lbs. (kN)) ","9188 (41.8)","7270 (32.3)","7300 (32.5)","7360 (32.7)","7360 (32.7)","12,907 (57.4)"]
["Cycle times"]
["Raise (seconds) ",5.1,3.6,3.5,3.9,4.5,4.18]
["Lower (seconds) ",3.5,1.8,2.3,2.5,2.6,2.18]
["Dump (seconds) ",2.7,2.2,2.6,2.7,2.6,2.25]
["Roll back (seconds) ",2,1.7,2,2,2,1.6]
["Weights"]
["Operating Weight  ","10,610 lbs (4813 kg)","8,270 lbs (3750 kg)","8,380 lbs (3810 kg)","9,630 lbs (4370 kg)","9,945 lbs (4520 kg)","16,100 lbs (7311 kg)"]
["Shipping weight (lbs. (kg)) ","10,267 (4657)","7970 (3615)","8080 (3673)","9300 (4220)","9615 (4370)","15,800 (7182)"]
["Service Capacities"]
["Fuel tank (gal. (L)) ","25.5 (96.5)","19.5 (73.8)","19.5 (73.8)","25.5 (96.5)","25.5 (96.5)","30.8 (116.5)"]
["Engine oil with filter (qt. (L)) ","8.9 (8.5)","8.9 (8.5)","7.5 (7.1)","8.9 (8.5)","8.9 (8.5)","8.9 (8.5)"]
["System Capacity with filter (qt. (L)) ","45.4 (48)","34 (32.2)","40.3 (38.1)","47 (44.5)","47 (44.5)","42.8 (40.5)"]
["DEF tank (gal. (L)) ","2.8 (10.7)","_","-","-","_","3.3 (12.4)"]
["Lift Style"]
["Lift design "]