{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":49,"n_cols":10,"rows_kept":49,"cut":false,"hidden":false,"merged":[]}
[]
[null,"ML35 Telescopic","ML12","ML12 Telescopic","ML15","ML22X","ML23","ML27","ML27 Telescopic","ML50 Telescopic"]
["Operating Weight"]
["Open cab (lbs. (kg)) ","8,818 (4000)","2,425 (1100)","2,646 (1200)",null,"4,850 (2200)","5,181 (2350)",null,null,"11,464 (5200)"]
["Overall Dimensions"]
["Overall height (in. (mm)) ","89.6 (2275)","81.1 (2060)","81.1 (2060)",null,"90.6 (2300)","90.6 (2300)",null,null,"99.3 (2523)"]
["Overall length: Without bucket (in. (mm)) ","160.1 (4067)","87.0 (2211)","89.2 (2265)",null,"120.2 (3054)","123.8 (3145)",null,null,"209.1 (5310)"]
["Machine width (in. (mm.))  ","52.8 (1340)","36.2 (920)","36.2 (920)",null,"48.4 (1230)","48.4 (1230)",null,null,"57.5 (1460)"]
["Loader Performance Specs"]
["Lifting height (in. (mm)) ","169.9 (4312)","85.4 (2170)","111.0 (2820)",null,"96.5 (2450)","96.5 (2450)",null,null,"171.3 (4350)"]
["Tipping load (ISO) - Straight (lb. (kg)) ",null,"2,205 (1000)","1,650 (750)",null,"4,528 (2054)","4,982 (2260)",null,null,"4,820 (2185)"]
["Lifting capacity (lb. (kg)) ","1,630 (740) to 5,510 (2500) depending on loader position","2,425 (1100)","440 to 1,650 (200 to 750) dependent on tipping load path",null,"4,850 (2200)","4,850 (2200)",null,null,"2,780 (1260) to 6,170 (2800) dependent on tipping load path"]
["Electrical"]
["System voltage  ","12 Volts","12 Volts","12 Volts",null,"48 Voltage Nominal Battery","12 Volts",null,null,"12 Volts"]
["Alternator ","60 Amp","40 Amp","40 Amp",null,"-","60 Amp",null,null,"60 Amp"]
["Battery  ","77 AHR\n520 Cold-Cranking Amps","52 AHR\n520 Cold-Cranking Amps","52 AHR 520 Cold-Cranking Amps",null,"Lithium Ion","52 AHR 520 Cold-Cranking Amps",null,null,"120 AHR\n1,000 Cold-Cranking Amps"]
["Engine"]
["Engine model ","Kubota V2403 CR","Kubota D902","Kubota D902",null,"-","Kubota V1505",null,null,"Kubota V3307 CR"]
["Emissions certification ","Tier 4 Final Certified","Tier 4 Final Certified","Tier 4 Final Certified",null,"-","Tier 4 Final Certified",null,null,"Tier 4 Final/Stage V"]
["Cylinders  ",4,3,3,null,"-",4,null,null,4]
["Displacement ","148.5 in.3 (2.434 L)","54.8 in³ (0.898 L)","54.8 in³ (0.898 L)",null,"-","91.4 in³ (1.498 L)",null,null,"203.3 in3 (3.331 L)"]
["Fuel ","Diesel","Diesel","Diesel",null,"-","Diesel",null,null,"Diesel"]
["Exhaust aftertreatment  ",null,"-","-",null,"-","-",null,null,"DOC + DPF"]
["Engine speeds: Rated - full load  ","2,700 RPM","3,600 RPM","3,600 RPM",null,"-","2,300 RPM",null,null,"2,600 RPM"]
["Horsepower @ 3,600 RPM – SAE J1349:  Gross (hp (kW)) ","65 (48.6)","25 (18.5)","25 (18.5)",null,"-","26 (19.4)",null,null,"74 HP (55.4)"]
["Peak torque (lb·ft (N·m)) ","146.4 lb·ft (198.5 N·m)","41.4 (56.1) @ 2,600 RPM","41.4 (56.1) @ 2,600 RPM",null,"-","68.3 (92.6) @ 2,200 RPM",null,null,"195.4 lb·ft (265.0 N·m @1,500 RPM"]
["Drivetrain"]
["Transmission type ","Hydrostatic, 2 speed","Hydrostatic","Hydrostatic",null,"Electric","Hydrostatic",null,null,"Hydrostatic,\n2+2 speed"]
["Differential type ","Open Center w/ Differential Lock","Hydraulic Controlled","Hydraulic Controlled",null,"Limited Slip","Limited Slip",null,null,"Open Center w/\nDifferential Lock"]
["Parking brake: Type ","Drum","Hydraulic Multidisk Brake","Hydraulic Multidisk Brake",null,"Drum","Drum",null,null,"Hydraulic Multidisc\nSAHR"]
["Max. travel speed (mph (kph)) ","18.6 (30)","9.3 (15)","9.3 (15)",null,"11.2 (18)","12.4 (20)",null,null,"21.6 (34.7)"]
["Hydraulics"]
["Control valve type ","Open Center","Open Center","Open Center",null,"Open Center","Open Center",null,null,"Open Center"]
["Pump type ","Fixed Gear","Fixed Gear","Fixed Gear",null,"Fixed Gear","Fixed Gear",null,null,"Fixed Gear"]
["Driving hydraulics: Flow rate (gpm (L/min)) ","29.6 (112)","17.2 (65)","17.2 (65)",null,"9.2 (35)","17.2 (65)",null,null,"38.3 (145)"]
["Driving hydraulics: Operating pressure (psi (bar)) ","6,500 (450)","5,100 (350)","5,100 (350)",null,"2,500 (170)","5,200 (360)",null,null,"7,000 (480)"]
["Working Hydraulics: Total flow rate (gpm (L/min)) ","18.5 (70)","7.4 (28)","7.4 (28)",null,"11.1 (42)","8.5 (32)",null,null,"20.6 (78)"]
["Working Hydraulics: Operating pressure (psi (bar)) ","3,200 (220)","2,200 (150)","2,200 (150)",null,"2,500 (170)","3,000 (210)",null,null,"3,600 (250)"]
["Auxiliary 1: Max. flow rate (gpm (L/min)) ","18.5 (70)","7.4 (28)","7.4 (28)",null,"9.2 (35)","8.5 (32)",null,null,"20.6 (78)"]
["Auxiliary 2 — optional: Max. flow rate (gpm (L/min)) ","18.5 (70)","7.4 (28)","7.4 (28)",null,"9.2 (35)","8.5 (32)",null,null,"20.6 (78)"]
["Auxiliary 1: Pressure (psi (bar)) ","3,200 (220)","2,200 (150)","2,200 (150)",null,"2,500 (170)","3,000 (210)",null,null,"3,600 (250)"]
["Auxiliary 2 — optional: Pressure (psi (bar)) ","3,200 (220)","2,200 (150)","2,200 (150)",null,"2,500 (170)","3,000 (210)",null,null,"3,600 (250)"]
["Continuous flow — optional: Max. flow rate (gpm (L/min)) ","13.2 (50)","10.3 (39)","10.3 (39)",null,"-","10.0 (38)",null,null,"35.7 (135)"]
["Continuous flow — optional: Pressure (psi (bar)) ","3,200 (220)","2,200 (150)","2,200 (150)",null,"-","3,000 (210)",null,null,"3,600 (250)"]
["Service Capacities "]
["Fuel tank (gal. (L))  ","18 (68)","11.9 (45)","11.9 (45)",null,"-","9.8 (37)",null,null,"20.3 (77)"]
["Engine oil w/ filter (qt. (L)) ","10 (9.5)","2.6 (2.5)","2.6 (2.5)",null,"-","5.4 (5.1)",null,null,"11.9 (11.3)"]
["Hydraulic system (gal. (L)) ","15.9 (60)","13.7 (52)","13.7 (52)",null,"6.6 (25)","14.8 (56)",null,null,"21.1 (80)"]
["Engine coolant (gal. (L)) ","3 (11.4)","1.1 (4.35)","1.1 (4.35)",null,"-","1.1 (4.4)",null,null,"3.3 (12.35)"]